; config options
server:
	access-control: 127.0.0.1 allow_snoop
	cache-min-ttl: 10
	qname-minimisation: "no"
	minimal-responses: no

stub-zone:
	name: "."
	stub-addr: 193.0.14.129 	# K.ROOT-SERVERS.NET.
CONFIG_END

SCENARIO_BEGIN Test TTL min option for messages in the cache

; K.ROOT-SERVERS.NET.
RANGE_BEGIN 0 100
	ADDRESS 193.0.14.129 
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
. IN NS
SECTION ANSWER
. IN NS	K.ROOT-SERVERS.NET.
SECTION ADDITIONAL
K.ROOT-SERVERS.NET.	IN	A	193.0.14.129
ENTRY_END

ENTRY_BEGIN
MATCH opcode subdomain
ADJUST copy_id copy_query
REPLY QR NOERROR
SECTION QUESTION
com. IN A
SECTION AUTHORITY
com.	IN NS	a.gtld-servers.net.
SECTION ADDITIONAL
a.gtld-servers.net.	IN 	A	192.5.6.30
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR AA NOERROR
SECTION QUESTION
a.gtld-servers.net.	IN A
SECTION ANSWER
a.gtld-servers.net.	IN A	192.5.6.30
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR AA NOERROR
SECTION QUESTION
K.ROOT-SERVERS.NET.	IN	A
SECTION ANSWER
K.ROOT-SERVERS.NET.	IN	A	193.0.14.129
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR AA NOERROR
SECTION QUESTION
a.gtld-servers.net.	IN AAAA
SECTION AUTHORITY
. 86400 IN SOA . . 20070304 28800 7200 604800 86400
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR AA NOERROR
SECTION QUESTION
K.ROOT-SERVERS.NET.	IN	AAAA
SECTION AUTHORITY
. 86400 IN SOA . . 20070304 28800 7200 604800 86400
ENTRY_END

RANGE_END

; a.gtld-servers.net.
RANGE_BEGIN 0 100
	ADDRESS 192.5.6.30
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
com. IN NS
SECTION ANSWER
com.	IN NS	a.gtld-servers.net.
SECTION ADDITIONAL
a.gtld-servers.net.	IN 	A	192.5.6.30
ENTRY_END

ENTRY_BEGIN
MATCH opcode subdomain
ADJUST copy_id copy_query
REPLY QR NOERROR
SECTION QUESTION
example.com. IN A
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END
RANGE_END

; ns.example.com.
RANGE_BEGIN 0 100
	ADDRESS 1.2.3.4
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
example.com. IN NS
SECTION ANSWER
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR AA NOERROR
SECTION QUESTION
ns.example.com. IN A
SECTION ANSWER
ns.example.com.		IN 	A	1.2.3.4
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
www.example.com. IN A
SECTION ANSWER
www.example.com.  5 IN A	10.20.30.40
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR AA NOERROR
SECTION QUESTION
ns.example.com. IN AAAA
SECTION AUTHORITY
example.com. 10 IN SOA . . 15 28800 7200 604800 10
ENTRY_END

RANGE_END

; start by passing time ; so we are not at 0
STEP 1 TIME_PASSES ELAPSE 10

; query for the record
STEP 8 QUERY
ENTRY_BEGIN
REPLY RD CD
SECTION QUESTION
www.example.com. IN A
ENTRY_END

STEP 10 CHECK_ANSWER
ENTRY_BEGIN
MATCH all ttl
REPLY QR RD RA CD
SECTION QUESTION
www.example.com. IN A
SECTION ANSWER
www.example.com. 10 IN A	10.20.30.40
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

; wait for 7 seconds
STEP 20 TIME_PASSES ELAPSE 7

; do a lookup to check TTLs.
STEP 25 QUERY
ENTRY_BEGIN
REPLY
SECTION QUESTION
www.example.com. IN A
ENTRY_END

STEP 26 CHECK_ANSWER
ENTRY_BEGIN
MATCH all ttl
REPLY QR RA
SECTION QUESTION
www.example.com. IN A
SECTION ANSWER
www.example.com. 3 IN A	10.20.30.40
SECTION AUTHORITY
example.com.	3593 IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.	3593 	IN 	A	1.2.3.4
ENTRY_END

SCENARIO_END
