; config options
server:
	target-fetch-policy: "0 0 0 0 0"
	qname-minimisation: "no"
	minimal-responses: no

	private-address: 10.0.0.0/8
	private-address: 172.16.0.0/12
	private-address: 192.168.0.0/16
	private-address: 169.254.0.0/16
	private-address: fd00::/8
	private-address: fe80::/10

	private-domain: "example.net"

stub-zone:
	name: "."
	stub-addr: 193.0.14.129 	# K.ROOT-SERVERS.NET.

CONFIG_END

SCENARIO_BEGIN Test iterator scrubber with private addresses.

; K.ROOT-SERVERS.NET.
RANGE_BEGIN 0 100
	ADDRESS 193.0.14.129 
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
. IN NS
SECTION ANSWER
. IN NS	K.ROOT-SERVERS.NET.
SECTION ADDITIONAL
K.ROOT-SERVERS.NET.	IN	A	193.0.14.129
ENTRY_END

ENTRY_BEGIN
MATCH opcode subdomain
ADJUST copy_id copy_query
REPLY QR NOERROR
SECTION QUESTION
com. IN A
SECTION AUTHORITY
com.	IN NS	a.gtld-servers.net.
SECTION ADDITIONAL
a.gtld-servers.net.	IN 	A	192.5.6.30
ENTRY_END

; root server authoritative for example.net too.
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
mail.example.net. IN A
SECTION ANSWER
mail.example.net. IN A 10.20.30.40
ENTRY_END
RANGE_END

; a.gtld-servers.net.
RANGE_BEGIN 0 100
	ADDRESS 192.5.6.30
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
com. IN NS
SECTION ANSWER
com.	IN NS	a.gtld-servers.net.
SECTION ADDITIONAL
a.gtld-servers.net.	IN 	A	192.5.6.30
ENTRY_END

ENTRY_BEGIN
MATCH opcode subdomain
ADJUST copy_id copy_query
REPLY QR NOERROR
SECTION QUESTION
example.com. IN A
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END
RANGE_END

; ns.example.com.
RANGE_BEGIN 0 100
	ADDRESS 1.2.3.4
ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
example.com. IN NS
SECTION ANSWER
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
ns.example.com. IN A
SECTION ANSWER
ns.example.com.		IN 	A	1.2.3.4
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
ns.example.com. IN AAAA
SECTION ANSWER
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
www.example.com. IN A
SECTION ANSWER
www.example.com. IN A	192.20.30.40
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
mail.example.com. IN AAAA
SECTION ANSWER
mail.example.com. IN AAAA fe80::15
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
foo.example.com. IN A
SECTION ANSWER
foo.example.com. IN A	10.20.30.40
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

ENTRY_BEGIN
MATCH opcode qtype qname
ADJUST copy_id
REPLY QR NOERROR
SECTION QUESTION
toss.example.com. IN A
SECTION ANSWER
toss.example.com. IN A	10.20.30.40
toss.example.com. IN A	1.2.3.4
toss.example.com. IN A	10.20.30.41
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END
RANGE_END

; public address is not scrubbed
STEP 1 QUERY
ENTRY_BEGIN
REPLY RD
SECTION QUESTION
www.example.com. IN A
ENTRY_END

; recursion happens here.
STEP 2 CHECK_ANSWER
ENTRY_BEGIN
MATCH all
REPLY QR RD RA NOERROR
SECTION QUESTION
www.example.com. IN A
SECTION ANSWER
www.example.com. IN A	192.20.30.40
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

; IPv4 address is scrubbed
STEP 3 QUERY
ENTRY_BEGIN
REPLY RD
SECTION QUESTION
foo.example.com. IN A
ENTRY_END

; recursion happens here.
STEP 10 CHECK_ANSWER
ENTRY_BEGIN
MATCH all
REPLY QR RD RA SERVFAIL
SECTION QUESTION
foo.example.com. IN A
SECTION ANSWER
; scrubbed away
;foo.example.com. IN A	10.20.30.40
ENTRY_END

; IPv6 address is scrubbed
STEP 20 QUERY
ENTRY_BEGIN
REPLY RD
SECTION QUESTION
mail.example.com. IN AAAA
ENTRY_END

STEP 30 CHECK_ANSWER
ENTRY_BEGIN
MATCH all
REPLY QR RD RA SERVFAIL
SECTION QUESTION
mail.example.com. IN AAAA
SECTION ANSWER
ENTRY_END

; allowed domain is not scrubbed.
STEP 40 QUERY
ENTRY_BEGIN
REPLY RD
SECTION QUESTION
mail.example.net. IN A
ENTRY_END

STEP 50 CHECK_ANSWER
ENTRY_BEGIN
MATCH all
REPLY QR RD RA NOERROR
SECTION QUESTION
mail.example.net. IN A
SECTION ANSWER
mail.example.net. IN A 10.20.30.40
ENTRY_END

; rest of RRset intact, only 10/8 tossed away.
STEP 60 QUERY
ENTRY_BEGIN
REPLY RD
SECTION QUESTION
toss.example.com. IN A
ENTRY_END

STEP 70 CHECK_ANSWER
ENTRY_BEGIN
MATCH all
REPLY QR RD RA NOERROR
SECTION QUESTION
toss.example.com. IN A
SECTION ANSWER
; toss.example.com. IN A	10.20.30.40
toss.example.com. IN A	1.2.3.4
SECTION AUTHORITY
example.com.	IN NS	ns.example.com.
SECTION ADDITIONAL
ns.example.com.		IN 	A	1.2.3.4
ENTRY_END

SCENARIO_END
